{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,6],[9,2,9,6],[10,1,10,6],[11,0,11,6]],"flags":["formulas_cached_only"]}
["济南市地震监测中心异常核实设备采购项目报价单"]
[{"$nulls":5},"日期：     年   月   日"]
["序号","设备名称","单位","数量","参数","单价（元）","合计\n（元）"]
[1,"便携式电子水位仪","套",2,"（1）测量深度：≥200m；\n（2）分辨率：测量分辨率达到毫米；\n（3）探头材质：耐腐蚀不锈钢；\n（4）供电方式：可采用电池供电；\n（5）使用环境：可在-30℃～+80℃正常使用；\n（6）探测到水面指示：探头到达井水水面时，可发出声光报警；\n（7）适用测井材质：适合所有材质井管的水位测量。"]
[2,"便携式高精度温度计","套",1,"（1）量程：0℃～100℃；\n（2）精度等级：优于0.1%F.S；\n（3）长期稳定性：≤0.1%F.S/年；\n（4）最大测量误差：≤0.05℃；\n（5）分辨率：优于0.0001℃；\n（6）供电方式：可采用电池供电；\n（7）显示方式：配置数据读取显示器，可以直接显示现场水温数据。"]
[3,"便携式二氧化碳仪","套",1,"（1）可在野外进行土壤及井泉二氧化碳气体浓度的测量；\n（2）测量范围: 0～100%；\n（3）重复性：≤1%；\n（4）示值引用误差：≤±2% FS；\n（5）零点漂移：≤±2% FS；\n（6）量程漂移：≤±2% FS；\n（7）配置仪器便携箱和气体及水样品采集套件。"]
[4,"便携式pH仪","套",1,"（1）测量范围：0～14；\n（2）分辨力：0.01。"]
[5,"便携式电导率仪","套",2,"（1）测量范围：0～1000ms/cm；\n（2）分辨力：1μs/cm。"]
[6,"激光测距仪","套",1,"（1）量程：≥2000m；\n（2）工作方式：望远镜式。"]
[null,"合  计","小写：                        大写："]
["说明","1.交付地点：济南市地震监测中心历城地震台（济南市历城区旅游路8577号）；\n2.合同履约期限：签订合同后30日内完成供货；\n3.质保期：质保三年（质保期内免费更换或10日内完成维修）；\n4.付款方式：报价含设备本身费用、运输费、税金等项目所有费用，验收合格后开具发票，30日内付全款；\n5.报价单及营业执照（复印件盖章）于2025年7月4日12时前一式三份密封送至或邮寄至济南市历城区旅游路8577号，联系人：张老师，电话：0531-66951975。                                                                      \n"]
["报价单位（盖章）：              法定代表人或授权代理人签字：                 电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}